**ALFA BOX UX1 FIRMWARE UPDATE INSTRUCTIONS**

STEP 1: UPDATING FIRMWARE ON ALFA BOX (3 minutes)

1. Connect Alfa box to the TV and Internet

2. Insert flash drive (polish / russian) with Alfa firmware

3. Connect Alfa box to power and start pressing “Menu” button right away, until you see a blue screen

4. On a blue screen select from the list “Upgrade tools” and press > (right arrow)

5. Select from the list “USB Bootstrap” and press > (right arrow)

6. Blue screen will appear with message “insert flash drive”. Press enter. Updating process will start.

7. Box will restart automatically after update completes

STEP 2: ADDING BOX TO SUBSCRIBEASY.COM (2 minute)

While box is updating, do the following

1. Insert SN into the system

2. Insert MAC address into the system in “Processor Number” field (ex. 00:1A:79:0F:F7:9E)

3. Select product model “Polish Alfa” / “Russian Alfa”

4. Save the box into the system (Services will automatically be added to the box)

STEP 3: CHECKING THE BOX

1. After box was added to the system check that appropriate (Polish/Russian) icons appear on the home screen.
2. Click on the service icon to check that the box is communicating with the system.
3. If you added box into the system Before updating process is completed, you will see icons with services right away.

If you added box After updating process was completed, you have to restart the box in order to see services on the home screen.